
[friendlyname]
Mercedes-Benz
O530 Citaro Manual Doors (3 Doors)
White

[description]
The Mercedes-Benz Citaro (coded as O530) is the current Mercedes-Benz/EvoBus mainstream single-decker bus intended for public transport, introduced in 1997 and replaced the Mercedes-Benz O405/O405N series.

-Technical data-

Length: 11950 mm
Width: 2550 mm
Height 3076 mm

Engine performance: 205 kW / 279 PS
Max speed: 91 km/h

Empty weight: 10.850 kg
Total weight: 18.000 kg

Seats: 30+2
Standing passengers: 75

More on omnibussimulator.ru
[end]

[number]
Regs_O530.org

	[registration_free]

[registration_automatic]
B-V 


[kmcounter_init]
1992
60000



[sound]
sound-citaro\sound_zf.cfg

[sound_ai]
sound-citaro\sound_zf.cfg

[model]
model\model_O530 3 Doors.cfg

[paths]
model\paths 3 Doors.cfg

[passengercabin]
model\passengercabin_O530 3 Doors.cfg

	////////////////////////////////////////////////////////
		Scripts
	////////////////////////////////////////////////////////

[varnamelist]
23
script\AI_varlist.txt
script\Collision_varlist.txt
script\antrieb_varlist_voith-zf.txt
script\engine_varlist.txt
script\elec_varlist.txt
script\bremse_varlist.txt
script\auspuff_varlist.txt
script\lights_varlist.txt
script\door_varlist_voith-zf.txt
script\wiper_varlist.txt
script\cockpit_varlist.txt
script\klappern_varlist.txt
script\rollband_varlist.txt
script\heizung_varlist.txt
script\rain_varlist.txt
script\dirt_varlist.txt
script\IBIS_varlist.txt
script\Matrix_varlist.txt
script\wimpel_varlist.txt
script\visual_varlist.txt
script\cashdesk_varlist.txt
script\ticketprinter_varlist.txt
script\Siemens VDO Panel_vars.txt

[stringvarnamelist]
4
script\IBIS_stringvarlist.txt
script\Matrix_stringvarlist.txt
script\ticketprinter_stringvarlist.txt
script\cockpit_stringvarlist.txt

[script]
29
script\man_D92_main.osc
script\man_D86_main_AI.osc
script\collision.osc
script\cockpit_voith-zf.osc
script\ZF-Ecomat-2.osc
script\engine.osc
script\elec.osc
script\bremse.osc
script\auspuff.osc
script\lights.osc
script\door_manual_voith-zf.osc
script\wiper.osc
script\klappern.osc
script\forcefeedback.osc
script\rain.osc
script\dirt.osc
script\sound_volume.osc
script\heizung.osc
script\IBIS-2.osc
script\matrix_D.osc
script\wimpel.osc
script\cashdesk.osc
script\ticketprinter.osc
script\summer.osc
script\Siemens VDO Panel.osc
script\Siemens VDO Disp1.osc
script\Siemens VDO Disp2.osc
script\Siemens VDO Disp3.osc
script\Siemens VDO Disp4.osc

[constfile]
19
script\AI_constfile.txt
script\collision_constfile.txt
script\zf-5hp-592.txt
script\engine_constfile_voith-zf.txt
script\elec_constfile.txt
script\bremse_constfile_D92.txt
script\lights_constfile.txt
script\door_constfile_o530.txt
script\auspuff_constfile.txt
script\cockpit_constfile_D92.txt
script\klappern_constfile.txt
script\rollband_constfile.txt
script\forcefeedback_constfile.txt
script\wiper_constfile.txt
script\dirt_constfile.txt
script\heizung_constfile.txt
script\IBIS_constfile.txt
script\matrix_constfile.txt
script\Siemens VDO Panel_const.txt



	////////////////////////////////////////////////////////
		Kameras *NEU01*
	////////////////////////////////////////////////////////

	0: Blick nach ganz links
[add_camera_driver]
-1.5
4.68
1.84
-0.06
55
-170
-5
	1: Blick nach schrдg links
[add_camera_driver]
-0.713
4.68
1.84
-0.06
55
-60
-5
	2: Blick in den linken Spiegel
[add_camera_driver]
-0.713
4.68
1.84
-0.06
55
-30
2

	3: Blick nach vorne (std)
[add_camera_driver]
-0.713
4.68
1.84
-0.06
55
0
-10




	4: Blick in den rechten Spiegel
[add_camera_driver]
-0.713
4.68
1.84
-0.06
55
33
10

	5: Blick zur Tьr
[add_camera_driver]
-0.713
4.68
1.84
-0.06
55
70
-10

	6: Fahrscheinverkauf-Sicht
[add_camera_driver]
-0.713
4.78
1.84
-0.06
50
60
-35

[view_ticketselling]


	7: Blick nach ganz rechts
[add_camera_driver]
0
4.68
1.78
-0.06
55
160
-10


	8: Panel-Zoom
[add_camera_driver]
-0.713
5
2.25
-0.06
55
5
-70

	7: Fahrplan-Sicht
[add_camera_driver]
-0.713
4.68
1.84
-0.06
55
-15
45
[view_schedule]



################
Passagiersichten
################

	0: Hinten links sitzend
[add_camera_pax]
-0.945
-2.185
2
-0.06
45
25
0

	1: Stehplatz an der Hintertuer
[add_camera_pax]
-0.8
-0.6
2.05
-0.06
45
90
0
	2: vorne rechts sitzend
[add_camera_pax]
0.94
1.67
1.6
-0.06
45
-20
0




	Folgender Befehl setzt die Standardfahrerkamera:

[set_camera_std]
3

	Folgender Befehl setzt den Zentrierpunkt der AuЯenkamera:

[set_camera_outside_center]
0
0
1.2



	////////////////////////////////////////////////////////
		Reflexionskameras *NEU01*
	////////////////////////////////////////////////////////
	
[add_camera_reflexion_2]
-1.348
5.56
2.2
0
52
169
-10
0.15

[add_camera_reflexion]
1.4
6.12
2.2
0
52
201
-10

[add_camera_reflexion]
0.266
4.92
2.508
0
52
210
-30

[add_camera_reflexion]
0.34
-0.69
2.4
0
52
30
-30



	////////////////////////////////////////////////////////
		Physikalische und geometrische Grunddaten
	////////////////////////////////////////////////////////

[mass]
12

500
200
500

[momentofintertia]
500
100
500

[boundingbox]
2.52
12
2.5
0
0.04
1.7

[cog]
0
0
0.8

[rollwiderstand]
1000

[rot_pnt_long]
-2.98

[inv_min_turnradius]
0.16

[ai_deltaheight]
-0.10

	Vorderachse:

[newachse]
achse_long
3.275
achse_maxwidth
2.4
achse_minwidth
1.83
achse_raddurchmesser
0.94
achse_feder
240
achse_maxforce
60
achse_daempfer
14
achse_antrieb
0

	Hinterachse:

[newachse]
achse_long
-2.615
achse_maxwidth
2.4
achse_minwidth
1.17
achse_raddurchmesser
0.94
achse_feder
280
achse_maxforce
116
achse_daempfer
14
achse_antrieb
1