
	[friendlyname]
Karosa
B941E - ZF - 5HP
Praha

[model]
model\2.cfg

[sound]
sound\sound_karosa_voith_zadekNormal.cfg

[sound_ai]
sound\sound_karosa_voith_zadekNormal.cfg

[scriptshare]

[paths]
model\paths_Trailer_B941E.cfg

[passengercabin]
model\passengercabin_B941E_Trailer.cfg

	////////////////////////////////////////////////////////
		Scripts
	////////////////////////////////////////////////////////

[varnamelist]
25
script\AI_varlist.txt
script\Collision_varlist.txt
script\antrieb_varlist_voith-zf.txt
script\engine_varlist_turbo.txt
script\elec_varlist.txt
script\bremse_varlist.txt
script\auspuff_varlist.txt
script\lights_varlist.txt
script\door_varlist85Mod_941.txt
script\wiper_varlist.txt
script\cockpit_varlist.txt
script\klappern_varlist.txt
script\heizung_varlist.txt
script\rain_varlist.txt
script\dirt_varlist.txt
script\OIS_varlist.txt
script\BUSE_varlist.txt
script\wimpel_varlist.txt
script\visual_varlist.txt
script\cashdesk_varlist.txt
script\ticketprinter_varlist.txt
script\okna_varlist.txt
script\JKZ_varlist.txt
script\MESIT_varlist.txt
script\articulation_varlist.txt

[stringvarnamelist]
7
script\OIS_stringvarlist.txt
script\BUSE_stringvarlist.txt
script\ticketprinter_stringvarlist.txt
script\cockpit_stringvarlist.txt
script\JKZ_stringvarlist.txt
script\DPP_stringvarlist.txt
script\MESIT_stringvarlist.txt
	////////////////////////////////////////////////////////
		Kameras *NEU01*
	////////////////////////////////////////////////////////


	0: Blick nach vorne (std)
[add_camera_driver]
0
4.68
1.84
-0.06
55
0
-10




################
Passagiersichten
################

	0: Hinten links sitzend
[add_camera_pax]
-0.5
-2.532
2.35
-0.06
55
25
0

	1: Stehplatz an der Hintertuer
[add_camera_pax]
0
-0.575
2.35
-0.06
55
90
0


	Folgender Befehl setzt die Standardfahrerkamera:

[set_camera_std]
3

	Folgender Befehl setzt den Zentrierpunkt der AuЯenkamera:

[set_camera_outside_center]
0
0
1.2


	////////////////////////////////////////////////////////
		Physikalische und geometrische Grunddaten
	////////////////////////////////////////////////////////

[mass]
6

500
200
500

[momentofintertia]
150
40
150

[boundingbox]
2.52
6.15
2.5
0
-0.32
1.7

[schwerpunkt]
1.2

[rollwiderstand]
500

[rot_pnt_long]
-0.675

[ai_deltaheight]
-0.10


	Hinterachse:

[newachse]
achse_long
-0.39
achse_maxwidth
2.4
achse_minwidth
1.17
achse_raddurchmesser
0.94
achse_feder
280
achse_maxforce
116
achse_daempfer
20
achse_antrieb
1

[coupling_front]
0
3.0
0.503

[couple_front_open_for_sound]

[coupling_front_character]
40.5
-20
20
1