[const]
engine_J
3.5

' Engine will automatically shutdown if RPM gets greater than this limit to prevent engine failure.

[const]
engine_rpm_limsup
3200

' Activates speed governor system (0 for disabled, 1 for enabled). Use curve
' Speed governor created by krtz07

[const]
speed_governor_sw
1

[const]
engine_speedcontrol
0

[const]
engine_e-gas
0

[const]
engine_ASR
0

[const]
engine_governed_idle_RPM
550

[const]
engine_power_idle
22710

[const]
engine_coldM
-300


############ SPEED LIMIT CURVE - by krtz07 ###########

[newcurve]
governor
[pnt]
-100.00
1

[pnt]
75.00
1

[pnt]
76.00
0

############ THROTTLE CURVE FOR MAX. INPUT ###########

[newcurve]
engine_M_maxThrottle_nom

[pnt]
50
0

[pnt]
300
250

[pnt]
592
520

[pnt]
600
780

[pnt]
1140
1027

[pnt]
1300
1027

[pnt]
1500
1027

[pnt]
1900
1027

[pnt]
2100
850

[pnt]
2200
400

[pnt]
2300
220

[pnt]
2500
0

############ THROTTLE CURVE FOR MIN. INPUT ###########

[newcurve]
engine_M_minThrottle_nom

[pnt]
50
0

[pnt]
300
250

[pnt]
550
0

[pnt]
650
-100

[pnt]
1900
-300

[pnt]
2800
-350

[pnt]
3000
-390


[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
300
400

[pnt]
592
500

[pnt]
600
500

[pnt]
1000
630

[pnt]
1400
700

[pnt]
1900
650

[pnt]
2100
641

[pnt]
2300
530

[pnt]
2350
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
250

[pnt]
550
0

[pnt]
650
-100

[pnt]
1000
-300

[pnt]
2500
-350

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
800
1

[pnt]
1200
0.45

[pnt]
1700
0.45

[pnt]
2300
0.2

[newcurve]
engine_efficiency_throttle

[pnt]
0
0.3

[pnt]
1
1

	mértékegység: g/kWh
[newcurve]
engine_consumption_per_rpm

[pnt]
0
228

[pnt]
800
226

[pnt]
1000
225

[pnt]
1100
224

[pnt]
1300
224

[pnt]
1560
225

[pnt]
1800
228

[pnt]
2100
234

[pnt]
3100
259

[const]
engine_consumption_curve_available
1

[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250


[const]
luefterthermostat_opn
92

[const]
luefterthermostat_cls
88

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
80

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
700

[const]
engine_Qrate_fan_factor
0.9

[const]
engine_Qrate_veloc_factor_basic
1500

[const]
engine_Qrate_veloc_factor
100

[const]
engine_cvm_engine
362000

[const]
engine_cvm_envir
50000

First is turbocharger PSI
Second is the torque mutipler
[newcurve]
turbo_M_max

[pnt]
0
0.65


[pnt]
30
1



[newcurve]
turbo_limit_thorttle_1

[pnt]
0
0


[pnt]
1
30

Controls the turbo boost using the engine rpm 
[newcurve]
turbo_engine_rpm_efficiency


[pnt]
550
0.50

[pnt]
950
1.00


[newcurve]
turbo_engine_rpm_max_psi
[pnt]
500
1

[pnt]
1000
30


[newcurve]
turbo_inertia

[pnt]
0
2.5032709057897112989048465462411


[pnt]
30
13.509812717369133896714539638723

[newcurve]
turbo_inertia_dec

[pnt]
0
1
[pnt]
5
2

[pnt]
10
5

[pnt]
30
30

[newcurve]
turbo_M_inertia_throttle

[pnt]
0
0


[pnt]
1
1


[newcurve]
engine_airflow

[pnt]
0
1

[pnt]
20
2