[const]
engine_J
3.5

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_ASR
0

[const]
speedgov
97


[const]
rpmgov
2400

[const]
engine_governed_idle_RPM
575

[const]
engine_power_idle
15124

[const]
engine_coldM
-300

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
300
400

[pnt]
592
500

[pnt]
600
500

[pnt]
1000
680

[pnt]
1200
850

[pnt]
1800
850

[pnt]
2100
740

[pnt]
2300
670

[pnt]
2350
0


[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
250

[pnt]
592
0

[pnt]
650
-100

[pnt]
1000
-300

[pnt]
2500
-350

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
0.6

[pnt]
1200
0.45

[pnt]
1700
0.45

[pnt]
2300
0.2

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1

[newcurve]
engine_braking

[pnt]
0
1

[pnt]
1
0



[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250



[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000


First is turbocharger PSI
Second is the torque mutipler
[newcurve]
turbo_M_max

[pnt]
0
0.67


[pnt]
30
1



[newcurve]
turbo_limit_thorttle_1

[pnt]
0
0

[pnt]
1
30

Controls the turbo boost using the engine rpm 
[newcurve]
turbo_engine_rpm_efficiency


[pnt]
550
0.5

[pnt]
1000
1.00


[newcurve]
turbo_engine_rpm_max_psi
[pnt]
500
0

[pnt]
750
30


[newcurve]
turbo_inertia

[pnt]
0
3

[pnt]
10
30

[pnt]
30
90

[newcurve]
turbo_inertia_dec

[pnt]
0
0.5


[pnt]
30
30

[newcurve]
turbo_M_inertia_throttle

[pnt]
0
0


[pnt]
1
1


[newcurve]
governor
[pnt]
0
1

[pnt]
1
0

[pnt]
1.01
-0.01




[newcurve]
rpmgov_map

[pnt]
-25
1

[pnt]
0
0




[newcurve]
engine_airflow

[pnt]
0
1


[pnt]
10
2