'######################
' MAN D2566UH
'######################

' Engine Inertia

[const]
engine_J
2.8

' Engine will automatically shutdown if RPM gets greater than this limit to prevent engine failure.

[const]
engine_rpm_limsup
3500

' Activates speed governor system (0 for disabled, 1 for enabled). Use curve
' Speed governor created by krtz07

[const]
speed_governor_sw
1

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_ASR
0

' Engine IDLE RPM

[const]
engine_governed_idle_RPM
650

' Engine Power at Idle

[const]
engine_power_idle
22710

' ???

[const]
engine_coldM
-300

############ SPEED LIMIT CURVE - by krtz07 ###########

[newcurve]
governor
[pnt]
-100.00
1

[pnt]
105.00
1

[pnt]
120
0


############ THROTTLE CURVE FOR MIN. INPUT ###########

[newcurve]
engine_M_minThrottle_nom

[pnt]
50
0

[pnt]
300
250

[pnt]
592
0

[pnt]
650
-100

[pnt]
1000
-300

[pnt]
3200
-350

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
300
400

[pnt]
700
450

[pnt]
1000
455

[pnt]
1500
460

[pnt]
1800
470

[pnt]
2000
465

[pnt]
2500
455

[pnt]
3100
400

[pnt]
3250
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
50

[pnt]
880
0

[pnt]
1000
-50

[pnt]
1100
-100

[pnt]
3200
-150

############ EFFICIENCY CURVE X RPM ###########

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
0.2

[pnt]
1200
0.35

[pnt]
1800
0.55

[pnt]
3100
0.2

############ EFFICIENCY CURVE X THROTTLE INPUT ###########

[newcurve]
engine_efficiency_throttle

[pnt]
0
0.8

[pnt]
0.8
1

[pnt]
1
1.05

[newcurve]
engine_consumption_per_rpm

[pnt]
0
228

[pnt]
800
226

[pnt]
1000
225

[pnt]
1100
224

[pnt]
1300
224

[pnt]
1560
225

[pnt]
1800
228

[pnt]
2100
234

[pnt]
3100
259

[const]
engine_consumption_curve_available
1

[const]
engine_fuel_value
12
8.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
105


[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
99
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
2.2

[const]
engine_Qrate_cooling_factor
155

[const]
engine_Qrate_fan_factor
1.05

[const]
engine_Qrate_veloc_factor_basic
155

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000

[newcurve]
engine_power_temp

[pnt]
0
1

[pnt]
95
1

[pnt]
125
0

[newcurve]
engine_moment_gang

[pnt]
-1
3

[pnt]
0
1

[pnt]
1
3

[pnt]
2
1

[pnt]
3
1

[pnt]
4
1

[pnt]
5
1

[pnt]
6
1

[pnt]
7
1