[const]
engine_J
5.0

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_ASR
1

[const]
engine_governed_idle_RPM
600

[const]
engine_power_idle
32000

[const]
engine_coldM
-305

[newcurve]
engine_n_coldM

[pnt]
0
-140

[pnt]
1300
-310

[pnt]
2500
-300

[const]
engine_oelvis_M_nulldeg
-20

[const]
engine_oelvis_M_expfactor
-0.05

[const]
engine_RPM_ign_cold
150

[const]
engine_RPM_ign_warm
150

	Zeit [s], wie lange er "orgelt", wenn er gerade so die untere, "warme" Grenzdrehzahl erreicht:

[const]
engine_RPM_ign_time2warm
280


[const]
engine_starterM
1300

[const]
engine_starter_n_halbwert
67

[const]
engine_startering_sound_n_max
450

Mindeststrom, der immer durch den Starter fließt

[const]
engine_starter_minI
300

Ampere/Nm:

[const]
engine_starter_Ifaktor
0.5


[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
400
500

[pnt]
600
700

[pnt]
700
868

[pnt]
850
925

[pnt]
1000
1050

[pnt]
1200
1195

[pnt]
1420
1220

[pnt]
2100
950

[pnt]
2250
780

[pnt]
2350
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
300

[pnt]
450
500

[pnt]
507
0

[pnt]
900
-200

[pnt]
1000
-250

[pnt]
2000
-280

[pnt]
2800
-320

[newcurve]
engine_M_brake

[pnt]
50
0

[pnt]
300
0

[pnt]
565
0

[pnt]
600
-420

[pnt]
2000
-520

[const]
engine_brake_only_with_hard_gear
0

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
550
1

[pnt]
1200
0.45

[pnt]
1700
0.45

[pnt]
2200
0.2

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2

[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250


[const]
luefterthermostat_opn
82

[const]
luefterthermostat_cls
79

[const]
kuehlerthermostat_opn
81

[const]
kuehlerthermostat_cls
77

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
380

[const]
engine_Qrate_fan_factor
1.4

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_kalyha
3600000

[const]
engine_cvm_envir
10000


First is turbocharger PSI
Second is the torque mutipler
[newcurve]
turbo_M_max

[pnt]
0
0.85

[pnt]
35
1.1320

[newcurve]
turbo_limit_thorttle_1

[pnt]
0
5

[pnt]
1
35

[newcurve]
turbo_engine_rpm_min_psi

[pnt]
250
0

[pnt]
800
11

[pnt]
1200
15

[pnt]
2100
20

[newcurve]
turbo_engine_rpm_max_psi

[pnt]
200
0

[pnt]
500
12

[pnt]
1000
18

[pnt]
1500
25

[pnt]
2100
35

[newcurve]
turbo_inertia

[pnt]
0
4

[pnt]
30
6

[newcurve]
turbo_inertia_dec

[pnt]
0
1

[pnt]
5
2

[pnt]
10
4

[pnt]
30
6

[newcurve]
turbo_M_inertia_throttle

[pnt]
0
1


[pnt]
1
1


[newcurve]
engine_airflow

[pnt]
0
1

[pnt]
20
2