Alle Spannungen normiert!

[const]
elec_Vnenn
28


	Duration the battery will need to decrease its voltage to zero [s]:

[const]
elec_generator_minRPM
350



[const]
elec_battery_anteil_InnenT
0.2


[const]
elec_V_generator_max
1.000


[const]
elec_busbar_minV
0.4


Q in Ampere-Stunden:
[const]
elec_battery_Q
135

[const]
elec_battery_I_maxloading
-4

[newcurve]
elec_battery_load-V

[pnt]
0
0.8493

[pnt]
0.25
0.8614

[pnt]
0.5
0.8743

[pnt]
0.75
0.8893

[pnt]
1
0.9036



[newcurve]
elec_battery_T-FactRi

[pnt]
-60
7

[pnt]
-20
3

[pnt]
-10
2

[pnt]
0
1.25

[pnt]
10
1


C: I / (Q/1h), also man teile den Strom in A durch die Kapazitäts-Zahl in Ah:

[newcurve]
elec_battery_C-AhFaktor

[pnt]
0.2
1.0

[pnt]
0.28
0.84

[pnt]
0.6
0.6

[pnt]
1.0
0.5



[newcurve]
elec_battery_T-Q

[pnt]
-20
0.1

[pnt]
-10
0.6

[pnt]
0
0.9

[pnt]
10
1.0



[newcurve]
elec_battery_load-Ri

[pnt]
-1
1.0

[pnt]
0
0.016

[pnt]
0.1
0.014

[pnt]
0.3
0.012

[pnt]
0.6
0.0112

[pnt]
1
0.0110
