[const]
engine_J
3.5

[const]
Exhaust_brake_enabled
1

[newcurve]
Exhaust_brake

[pnt]
650
-50

[pnt]
2500
-350


[const]
engine_consumption_curve_available
1

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_ASR
1

1=default
2=automotive throttle 50 percent equals 50 percent engine torque 
[const]
throttle_type
2

--------------------------------------------------------------------------
Turbocharger controls
--------------------------------------------------------------------------


2 enables the puff limiter/smoke contol most diesels has this enabled. 
[const]
turbochaged
1

[const]
smoke_limiter
0.6

Standard Turbochargers spools way slower then the VGT turbochargers
[const]
VGT_turbochager
1


--------------------------------------------------------------------------
Turbocharger Dynamics
--------------------------------------------------------------------------


Number of liters the engine has (CID) 
this helps calculate the spool rate
of the turbocharger

[const]
engine_CID
12.1



[const]
engine_volumetric_efficiency
90

Value in mm
[const]
turbo_compressor_wheel_size
70


[const]
turbo_min_psi
-1


[const]
turbo_max_psi
24.4045285


Pressure Ratio starts at 1:1, so an second  value at 0 would yield a pressure ratio of 1:1 or 14.7 PSI Non Aspirate Pressure with 0 PSI turbocharge boost.

Mutipler

[newcurve]
turbo_boost_threshold


[pnt]
500
0.59322033898

[pnt]
1000
1



[newcurve]
turbo_exhaust_flow

[pnt]
50
-1

[pnt]
150
6.29

[pnt]
200
10.29

[pnt]
300
19.11

[pnt]
400
26.46

[pnt]
600
44.1

--------------------------------------------------------------------------
RPM and Speed Governor controls
--------------------------------------------------------------------------


[const]
rpmgov_unload
2600


[const]
rpmgov
2600

[const]
engine_governed_idle_RPM
650


[newcurve]
idle_ctr

[pnt]
-50
1


[pnt]
50
0




[newcurve]
rpmgov_map

[pnt]
-50
1

[pnt]
0
0

Units in kph

[const]
speedgov
152

--
throttle control
--
[newcurve]
engine_throttle_sensitivity

[pnt]
0
0


[pnt]
1
1


------------------------
Speed Governor thershold 
------------------------

[newcurve]
governor


[pnt]
0
1

[pnt]
1
0

[pnt]
1.01
0





--------------------------------------------------------------------------
Performance Data units in NM
--------------------------------------------------------------------------


[newcurve]
engine_M_maxThrottle

[pnt]
300
500

[pnt]
592
625

[pnt]
600
800

[pnt]
900
1005

[pnt]
1300
1005

[pnt]
1900
750


[pnt]
2200
662

[pnt]
2600
610

[pnt]
3000
0




[newcurve]
engine_M_minThrottle


[pnt]
700
-65

[pnt]
800
-126


[pnt]
1000
-190

[pnt]
2400
-294.51


[pnt]
3000
-318



[const]
engine_coldM
-310


--------------------------------------------------------------------------
Fuel Performance Data
--------------------------------------------------------------------------


[newcurve]
engine_consumption_per_rpm

[pnt]
0
0

[pnt]
0
120


[pnt]
800
195


[pnt]
1100
190


[pnt]
1900
211


[pnt]
2800
255

[pnt]
4800
415


[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
1




[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2



[const]
engine_fuel_value
11.8
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250


--------------------------------------------------------------------------
Engine Cooling Data
--------------------------------------------------------------------------

[const]
luefterthermostat_opn
93

[const]
luefterthermostat_cls
87


Thermostat Open Temperature 
[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

Thermostat Open Temperature 




[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
600

[const]
engine_Qrate_fan_factor
1.55

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
1180000

[const]
engine_cvm_envir
10000

















[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100



[newcurve]
torquelimit

[pnt]
90
1850

[pnt]
105
850

[pnt]
130
300
