[const]
engine_J
5.5

[const]
engine_speedcontrol
0

[const]
engine_e-gas
0

[const]
engine_ASR
1

[const]
engine_governed_idle_RPM
520

[const]
engine_power_idle
25600

[const]
engine_coldM
-335

[newcurve]
engine_n_coldM

[pnt]
0
-140

[pnt]
1300
-310

[pnt]
2500
-300

[const]
engine_oelvis_M_nulldeg
-20

[const]
engine_oelvis_M_expfactor
-0.05

[const]
engine_RPM_ign_cold
150

[const]
engine_RPM_ign_warm
100

	Zeit [s], wie lange er "orgelt", wenn er gerade so die untere, "warme" Grenzdrehzahl erreicht:

[const]
engine_RPM_ign_time2warm
250


[const]
engine_starterM
1350

[const]
engine_starter_n_halbwert
67

[const]
engine_startering_sound_n_max
450

Mindeststrom, der immer durch den Starter fließt

[const]
engine_starter_minI
300

Ampere/Nm:

[const]
engine_starter_Ifaktor
0.5


[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
300
550

[pnt]
565
800

[pnt]
770
950

[pnt]
1000
1000

[pnt]
1200
1118

[pnt]
1735
1050

[pnt]
2000
970

[pnt]
2100
840

[pnt]
2300
600

[pnt]
2350
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
200

[pnt]
450
500

[pnt]
510
0

[pnt]
900
-280

[pnt]
1000
-300

[pnt]
2500
-320

[pnt]
2800
-360

[newcurve]
engine_M_brake

[pnt]
50
0

[pnt]
300
0

[pnt]
565
0

[pnt]
600
-350

[pnt]
2000
-550

[const]
engine_brake_only_with_hard_gear
0

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
800
1

[pnt]
1200
0.45

[pnt]
1700
0.45

[pnt]
2300
0.2

[newcurve]
engine_efficiency_throttle

[pnt]
0
0.7

[pnt]
0.8
0.9

[pnt]
1
1.15

[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250


[const]
luefterthermostat_opn
85

[const]
luefterthermostat_cls
80

[const]
kuehlerthermostat_opn
82

[const]
kuehlerthermostat_cls
80

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
425

[const]
engine_Qrate_fan_factor
1.4

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
500000

[const]
engine_cvm_kalyha
3600000

[const]
engine_cvm_envir
10000


First is turbocharger PSI
Second is the torque mutipler
[newcurve]
turbo_M_max

[pnt]
0
0.7

[pnt]
14
0.9

[pnt]
35
1.1256

[newcurve]
turbo_limit_thorttle_1

[pnt]
0
5

[pnt]
1
35

[newcurve]
turbo_engine_rpm_min_psi

[pnt]
200
0

[pnt]
500
0

[pnt]
800
5

[pnt]
1200
7

[pnt]
2100
10

[newcurve]
turbo_engine_rpm_max_psi

[pnt]
200
0

[pnt]
500
8

[pnt]
1000
18

[pnt]
1500
28

[pnt]
2100
35

[newcurve]
turbo_inertia

[pnt]
0
1

[pnt]
10
2

[pnt]
15
4

[newcurve]
turbo_inertia_dec

[pnt]
0
1

[pnt]
5
3

[pnt]
10
5

[pnt]
30
7

[newcurve]
turbo_M_inertia_throttle

[pnt]
0
1


[pnt]
1
1


[newcurve]
engine_airflow

[pnt]
0
1

[pnt]
20
2