	Front/Back Door Acceleration (100%/sē)

[const]
fdoor_acc
1.0

[const]
bdoor_acc
1.1

[const]
fdoor_acc2L
1.2

[const]
fdoor_acc2R
1.1

[const]
fdoor_acc3L
1.3

[const]
fdoor_acc3R
1.2

[const]
fdoor_acc4L
1.1

[const]
fdoor_acc4R
1.4

	Door Acceleration Variation (100%/sē)

[const]
door_acc_var
0.0

[const]
door_acc_var2L
0.0

[const]
door_acc_var2R
0.0

[const]
door_acc_var3L
0.0

[const]
door_acc_var3R
0.0

[const]
door_acc_var4L
0.0

[const]
door_acc_var4R
0.0

	Front/Back Door Max Speed (100%/s)

[const]
fdoor_maxspeed
1

[const]
fdoor_maxspeed2L
1

[const]
fdoor_maxspeed2R
1

[const]
fdoor_maxspeed3L
1

[const]
fdoor_maxspeed3R
1

[const]
fdoor_maxspeed4L
1

[const]
fdoor_maxspeed4R
1

[const]
bdoor_maxspeed
1

[const]
door_maxspeed_var
1

[const]
door_maxspeed_var2L
1

[const]
door_maxspeed_var2R
1

[const]
door_maxspeed_var3L
1

[const]
door_maxspeed_var3R
1

[const]
door_maxspeed_var4L
1

[const]
door_maxspeed_var4R
1

	Door Stop Reflexion Coefficient

[const]
door_refl
0.1

[const]
door_refl2L
0.1

[const]
door_refl2R
0.1

[const]
door_refl3L
0.1

[const]
door_refl3R
0.1

[const]
door_refl4L
0.1

[const]
door_refl4R
0.1

	Automatic Back Door Time

[const]
doorAftOpenTime
3

	Busstop Brake will only be activated belov MaxKMH:

[const]
Door_Bremse_Halte_MaxKMH
2

[const]
door_druckluft
1

[const]
door_needs_stopbrake
0

[const]
electric_doors
0

[newcurve]
door_0_opn_speed

[pnt]
0
90.2

[pnt]
0.2
90.7

[pnt]
0.8
90.7

[pnt]
0.85
90.1

[pnt]
0.95
90.1

[pnt]
1
0.4

[newcurve]
door_0_cls_speed

[pnt]
0
90.5

[pnt]
0.1
90.07

[pnt]
0.25
90.07

[pnt]
0.3
90.8

[pnt]
1
90.9

[newcurve]
door_1_opn_speed

[pnt]
0
90.42

[pnt]
0.2
90.92

[pnt]
0.8
90.92

[pnt]
10.85
90.07

[pnt]
10.95
90.07

[pnt]
1
0.4

[newcurve]
door_1_cls_speed

[pnt]
0
190.5

[pnt]
0.1
190.07

[pnt]
0.2
190.07

[pnt]
0.3
190.8

[pnt]
1
190.9




[newcurve]
door_2L_opn_speed

[pnt]
0
200.2

[pnt]
0.2
200.7

[pnt]
0.8
200.7

[pnt]
0.85
200.01

[pnt]
0.95
200.01

[pnt]
1
0.4

[newcurve]
door_2L_cls_speed

[pnt]
0
120.5

[pnt]
0.1
120.07

[pnt]
0.25
120.07

[pnt]
0.3
120.8

[pnt]
1
120.9



[newcurve]
door_2R_opn_speed

[pnt]
0
200.2

[pnt]
0.2
200.6

[pnt]
0.8
200.6

[pnt]
0.85
200.05

[pnt]
0.95
200.05

[pnt]
1
0.5

[newcurve]
door_2R_cls_speed

[pnt]
0
120.5

[pnt]
0.1
120.05

[pnt]
0.25
120.05

[pnt]
0.3
120.7

[pnt]
1
120.8



[newcurve]
door_3L_opn_speed

[pnt]
0
90.42

[pnt]
0.2
90.92

[pnt]
0.8
90.92

[pnt]
10.85
90.07

[pnt]
10.95
90.07

[pnt]
1
0.4

[newcurve]
door_3L_cls_speed

[pnt]
0
190.5

[pnt]
0.1
190.07

[pnt]
0.2
190.07

[pnt]
0.3
190.8

[pnt]
1
190.9



[newcurve]
door_3R_opn_speed

[pnt]
0
200.2

[pnt]
0.2
200.7

[pnt]
0.8
200.7

[pnt]
0.85
200.01

[pnt]
0.95
200.01

[pnt]
1
0.4

[newcurve]
door_3R_cls_speed

[pnt]
0
120.5

[pnt]
0.1
120.07

[pnt]
0.25
120.07

[pnt]
0.3
120.8

[pnt]
1
120.9

[newcurve]
door_4L_opn_speed

[pnt]
0
90.42

[pnt]
0.2
90.92

[pnt]
0.8
90.92

[pnt]
10.85
90.07

[pnt]
10.95
90.07

[pnt]
1
0.4

[newcurve]
door_4L_cls_speed

[pnt]
0
190.5

[pnt]
0.1
190.07

[pnt]
0.2
190.07

[pnt]
0.3
190.8

[pnt]
1
190.9



[newcurve]
door_4R_opn_speed

[pnt]
0
200.2

[pnt]
0.2
200.7

[pnt]
0.8
200.7

[pnt]
0.85
200.01

[pnt]
0.95
200.01

[pnt]
1
0.4

[newcurve]
door_4R_cls_speed

[pnt]
0
120.5

[pnt]
0.1
120.07

[pnt]
0.25
120.07

[pnt]
0.3
120.8

[pnt]
1
120.9