------------------------------------------------
'korekta pętli prędkościomierza (c)vanedek
-------------------------------------------------
[newcurve]
cockpit_tacholinie

[pnt]
0
0
[pnt]
5
0
[pnt]
10
10
[pnt]
20
23
[pnt]
30
48
[pnt]
40
75
[pnt]
50
100
[pnt]
60
127
[pnt]
70
154
[pnt]
80
181
[pnt]
90
208
[pnt]
100
235
[pnt]
110
262
[pnt]
120
289

------------------------------------
' obrotomierz (c)vanedek
------------------------------------

[newcurve]
cockpit_toltes

[pnt]
0
0

[pnt]
300
0.5

[pnt]
600
0.87

[pnt]
1000
1.5

[pnt]
1500
3.0

[pnt]
2000
5.1

[pnt]
2500
7.25

[pnt]
2800
9

[newcurve]
cockpit_oeldruck

[pnt]
300
0

[pnt]
400
1.1

[pnt]
1700
4.5

[newcurve]
odometer_10er-uebertrag
[pnt]
0
0
[pnt]
0.9
0
[pnt]
0.95
0.5
[pnt]
1
1

[newcurve]
cockpit_engine_temperature

[pnt]
0
0

[pnt]
60
17

[pnt]
70
29

[pnt]
80
45

[pnt]
90
65

[pnt]
100
84

[pnt]
110
100

[const]
automatic_battery_switch
1

[const]
auxheat_via_button
0

[const]
wiper_lever
0

[newcurve]
cockpit_warndruck

[pnt]
550000
1

[pnt]
700000
0

[const]
cockpit_gangwahltaster_alt
0

[const]
cockpit_zentralschmierung_dist
50

[const]
cockpit_zentralschmierung_maxtime
30

[const]
cockpit_gear_D_only
0

[const]
cockpit_has_20h_switch
1

[const]
cockpit_has_retarderswitch
0

[const]
cockpit_has_coolingswitch
0

[const]
cp_fahrertuer_anschlagseite
-1

[const]
eng_vent_spd_denominator
2