[newcurve]
cockpit_tacholinie

[pnt]
0
0
[pnt]
5
0
[pnt]
10
7
[pnt]
20
30
[pnt]
30
52
[pnt]
40
74
[pnt]
50
97
[pnt]
60
120
[pnt]
70
142
[pnt]
80
164
[pnt]
90
185
[pnt]
100
208
[pnt]
110
229
[pnt]
120
252

[newcurve]
cockpit_battery_voltage_line

[pnt]
0
0

[pnt]
0.74
26

[pnt]
0.888
40

[pnt]
0.9629
47

[pnt]
1.037
55

[pnt]
1.11
68

[pnt]
1.19
90

[newcurve]
cockpit_revlinie

[pnt]
0
0
[pnt]
290
0
[pnt]
300
9.2
[pnt]
500
18.5
[pnt]
600
27.3
[pnt]
700
36
[pnt]
900
54.2
[pnt]
1200
82.3
[pnt]
1500
110
[pnt]
1700
127
[pnt]
2000
154.2
[pnt]
2300
185
[pnt]
2600
211
[pnt]
2800
229
[pnt]
3000
246.6

[newcurve]
cockpit_oeldruck

[pnt]
300
0

[pnt]
400
0.9

[pnt]
1700
3.7

[newcurve]
odometer_10er-uebertrag
[pnt]
0
0
[pnt]
0.9
0
[pnt]
1
1

[newcurve]
cockpit_engine_temperature

[pnt]
0
0

[pnt]
40
2.5

[pnt]
60
21.2

[pnt]
70
27

[pnt]
80
32

[pnt]
90
49.2

[pnt]
100
65.3

[pnt]
110
83

[const]
automatic_battery_switch
1

[const]
auxheat_via_button
1

[const]
wiper_lever
0

[newcurve]
cockpit_warndruck

[pnt]
550000
1

[pnt]
700000
0

[const]
cockpit_gangwahltaster_alt
0

[const]
cockpit_zentralschmierung_dist
50

[const]
cockpit_zentralschmierung_maxtime
30

[const]
cockpit_gear_D_only
0

[const]
cockpit_has_20h_switch
0

[const]
cockpit_has_retarderswitch
1

[const]
cockpit_has_coolingswitch
1

[const]
cp_fahrertuer_anschlagseite
1

[const]
HH_funkpiep_active
1


=============================================
Inverse Widerstände (Leitwerte) in 1/Ohm.


Allgemeiner Stromverbrauch Panel (sonstige): 1x40W (1x0.0174 1/Ohm)

[const]
cp_general_Rinv
0.0174

.............................

Frontheizgerät: 1x60W (1x0.104 1/Ohm)

[const]
cp_klimator_Rinv
0.104

.............................

Hintere Heizgeräte (zusammen): 60W (0.104 1/Ohm)

[const]
cp_cabinheater_Rinv
0.104
