
[friendlyname]
Mercedes-Benz
O530 CapaCity (Voith)
Hochbahn rot-weiss

[description]
The Hamburger Stadtbus Mercedes Benz CapaCity (coded as O530 G) is the current Hamburger Stadtbus/EvoBus mainstream single-decker bus intended for public transport, introduced in 1997 and replaced the Hamburger Stadtbus O405/O405N series.

-Technical data-

Length: 19540 mm
Width: 2550 mm
Height 3076 mm

Engine performance: 260 kW / 354 PS
Max speed: 88 km/h

Empty weight: 18.548 kg
Total weight: 32.000 kg

Seats: 49+2
Standing passengers: 141

[end]

[number]
Regs_O530.org

	[registration_free]

[registration_automatic]
HH-X 


[kmcounter_init]
2006
1000



[sound]
sound-citaro\sound_om457hla.cfg

[sound_ai]
sound-citaro\sound_om457hla.cfg

[model]
model\model_O530 G_XL.cfg

[paths]
model\paths Main.cfg

[passengercabin]
model\passengercabin_O530 Main.cfg

	////////////////////////////////////////////////////////
		Scripts
	////////////////////////////////////////////////////////

[varnamelist]
25
script\AI_varlist.txt
script\Collision_varlist.txt
script\antrieb_varlist_voith-zf.txt
script\engine_varlist.txt
script\elec_varlist.txt
script\bremse_varlist.txt
script\auspuff_varlist.txt
script\lights_varlist.txt
script\door_varlist.txt
script\wiper_varlist.txt
script\cockpit_varlist.txt
script\klappern_varlist.txt
script\rollband_varlist.txt
script\heizung_varlist.txt
script\rain_varlist.txt
script\dirt_varlist.txt
script\IBIS_varlist.txt
script\Matrix_varlist.txt
script\wimpel_varlist.txt
script\visual_varlist.txt
script\cashdesk_varlist.txt
script\ticketprinterhh_varlist.txt
script\Siemens VDO Panel_vars.txt
script\articulation_varlist.txt
script\spray_varlist.txt

[stringvarnamelist]
6
script\IBIS_stringvarlist.txt
script\Rollband_stringvarlist.txt
script\Matrix_stringvarlist.txt
script\ticketprinter_stringvarlist.txt
script\cockpit_stringvarlist.txt
script\Matrix_fontfile_stringvarlist.txt

[script]
32
script\man_D92_main.osc
script\man_D86_main_AI.osc
script\collision.osc
script\cockpit.osc
script\Voith_DIWA.osc
script\engine.osc
script\elec.osc
script\bremse.osc
script\auspuff.osc
script\lights.osc
script\door.osc
script\wiper.osc
script\klappern.osc
script\forcefeedback.osc
script\rain.osc
script\dirt.osc
script\sound_volume.osc
script\heizung.osc
script\IBIS-2.osc
script\matrix.osc
script\matrix_fontfile.osc
script\wimpel.osc
script\cashdesk.osc
script\ticketprinterhh.osc
script\summer.osc
script\Siemens VDO Panel.osc
script\Siemens VDO Disp1.osc
script\Siemens VDO Disp2.osc
script\Siemens VDO Disp3.osc
script\Siemens VDO Disp4.osc
script\articulation.osc
script\spray.osc

[constfile]
20
script\AI_constfile.txt
script\collision_constfile.txt
script\Voith_D864.5.txt
script\engine_constfile_voith-zf.txt
script\elec_constfile.txt
script\bremse_constfile_D92.txt
script\lights_constfile.txt
script\door_constfile_D92.txt
script\auspuff_constfile.txt
script\cockpit_constfile_D92.txt
script\klappern_constfile.txt
script\rollband_constfile.txt
script\forcefeedback_constfile.txt
script\wiper_constfile.txt
script\dirt_constfile.txt
script\heizung_constfile.txt
script\IBIS_constfile.txt
script\matrix_constfile_kompl_Vollmatrix.txt
script\Siemens VDO Panel_const.txt
script\articulation_constfile.txt


	////////////////////////////////////////////////////////
		Kameras *NEU01*
	////////////////////////////////////////////////////////

	0: Blick nach ganz links
[add_camera_driver]
-1.5
4.68
1.84
-0.06
55
-170
-5
	1: Blick nach schrдg links
[add_camera_driver]
-0.713
4.68
1.84
-0.06
55
-60
-5
	2: Blick in den linken Spiegel
[add_camera_driver]
-0.713
4.68
1.84
-0.06
55
-30
2

	3: Blick nach vorne (std)
[add_camera_driver]
-0.713
4.68
1.84
-0.06
55
0
-10




	4: Blick in den rechten Spiegel
[add_camera_driver]
-0.713
4.68
1.84
-0.06
55
33
10

	5: Blick zur Tьr
[add_camera_driver]
-0.713
4.68
1.84
-0.06
55
70
-10

	6: Fahrscheinverkauf-Sicht
[add_camera_driver]
-0.713
4.78
1.84
-0.06
50
60
-35

[view_ticketselling]


	7: Blick nach ganz rechts
[add_camera_driver]
0
4.68
1.78
-0.06
55
160
-10


	8: Panel-Zoom
[add_camera_driver]
-0.713
5
2.25
-0.06
55
5
-70

	7: Fahrplan-Sicht
[add_camera_driver]
-0.713
4.68
1.84
-0.06
55
-15
45
[view_schedule]



################
Passagiersichten
################

	1: Hinten links sitzend
[add_camera_pax]
-0.945
-2.185
2
-0.06
55
0
0

	1a: Hinten links gegen Fahrtrichtung
[add_camera_pax]
-0.6
-3.1
1.6
-0.06
55
180
0

	1b: Vorne links
[add_camera_pax]
0.6
-2.0
1.6
-0.06
55
0
0

	2: vorne rechts sitzend
[add_camera_pax]
0.94
1.67
1.6
-0.06
55
-20
0

	2a: vorne links gegen Fahrtrichtung
[add_camera_pax]
-0.6
3.0
1.7
-0.06
45
-180
0

	2b: vorne links
[add_camera_pax]
-0.9
0.8
1.6
-0.06
45
25
0

	3: vorne auf dem "Beifahrersitz"
[add_camera_pax]
0.6
3.6
2.0
-0.06
45
-20
0



	Folgender Befehl setzt die Standardfahrerkamera:

[set_camera_std]
3

	Folgender Befehl setzt den Zentrierpunkt der AuЯenkamera:

[set_camera_outside_center]
0
0
1.2



	////////////////////////////////////////////////////////
		Reflexionskameras *NEU01*
	////////////////////////////////////////////////////////
	
[add_camera_reflexion_2]
-1.348
5.56
2.2
0
52
169
-10
0.15

[add_camera_reflexion]
1.4
6.12
2.2
0
52
201
-10

[add_camera_reflexion_2]
0.266
4.92
2.508
0
52
210
-30
0.2

[add_camera_reflexion]
0.34
-0.69
2.4
0
52
30
-30



	////////////////////////////////////////////////////////
		Physikalische und geometrische Grunddaten
	////////////////////////////////////////////////////////

[mass]
8

500
200
500

[momentofintertia]
300
80
300

[boundingbox]
2.52
10.5
2.5
0
0.7
1.7

[schwerpunkt]
1.2

[rollwiderstand]
900

[rot_pnt_long]
-2.5

[inv_min_turnradius]
0.13

[ai_deltaheight]
-0.12

	Vorderachse:

[newachse]
achse_long
3.275
achse_maxwidth
2.4
achse_minwidth
1.83
achse_raddurchmesser
0.94
achse_feder
240
achse_maxforce
60
achse_daempfer
20
achse_antrieb
0

	Hinterachse:

[newachse]
achse_long
-2.615
achse_maxwidth
2.4
achse_minwidth
1.17
achse_raddurchmesser
0.94
achse_feder
280
achse_maxforce
116
achse_daempfer
20
achse_antrieb
0.5

[coupling_back]
0
-4.456
0.503

[couple_back]
MB_O530 G Trail_HHA_XL.bus
false
