[const]
engine_J
7

[const]
engine_speedcontrol
0

[const]
engine_e-gas
2

[const]
engine_ASR
0

[const]
engine_governed_idle_RPM
1184

[const]
engine_power_idle
45420

[const]
engine_coldM
-600

[newcurve]
engine_M_maxThrottle

[pnt]
100
0

[pnt]
600
800

[pnt]
1184
1000

[pnt]
1200
1000

[pnt]
2000
1260

[pnt]
2800
1320

[pnt]
3800
1300

[pnt]
4200
1282

[pnt]
4600
1060

[pnt]
4700
0

[newcurve]
engine_M_minThrottle

[pnt]
100
0

[pnt]
600
500

[pnt]
1184
0

[pnt]
1300
-200

[pnt]
2000
-600

[pnt]
5000
-700

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
1200
1.2

[pnt]
2400
0.9

[pnt]
3400
0.9

[pnt]
4600
0.4

[newcurve]
engine_efficiency_throttle

[pnt]
0
2.6

[pnt]
1.6
2

[pnt]
2
2.4

[const]
engine_fuel_value
8
4.95
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
500


[const]
luefterthermostat_opn
180

[const]
luefterthermostat_cls
174

[const]
kuehlerthermostat_opn
170

[const]
kuehlerthermostat_cls
164

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
210
0

[pnt]
230
200


[const]
engine_Qrate_engine_factor
2.4

[const]
engine_Qrate_cooling_factor
600

[const]
engine_Qrate_fan_factor
2.3

[const]
engine_Qrate_veloc_factor_basic
400

[const]
engine_Qrate_veloc_factor
8

[const]
engine_cvm_engine
1200000

[const]
engine_cvm_envir
20000

