[const]
engine_J
2.1

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_governed_idle_RPM
820

[const]
engine_power_idle
22710

[const]
engine_coldM
-300

[newcurve]
engine_M_maxThrottle

[pnt]
0
0

[pnt]
500
315

[pnt]
2500
558

[pnt]
4000
412

[pnt]
5000
155

[pnt]
5500
0

[newcurve]
engine_M_minThrottle

[pnt]
0
0

[pnt]
500
150

[pnt]
600
200

[pnt]
820
0

[pnt]
830
0

[pnt]
1000
-410

[pnt]
2500
-470

[pnt]
5500
-500

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
500
0.25

[pnt]
1000
0.3

[pnt]
1500
0.35

[pnt]
2000
0.25

[pnt]
2500
0.25

[pnt]
5000
0.25

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2

[const]
engine_fuel_value
10
10.0
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250



[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
100

[pnt]
115
120


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000