'##############
'Engine Script
'##############

'Simulates basic engine behaviour, fuel cunsumption and cooling circuit

'(c) 23.03.2009 Rüdiger Hülsmann
'(c) 09.08.2009 Marcel Kuhnt

'Script Version: 1.5
'Omsi release: 1.0

'Needs:
'- Antrieb
'- Heizung


'Revision History:
'- Marcel Kuhnt		09.08.2009	Added Engine Failure
'- Marcel Kuhnt		10.08.2009	Added Revision History
'- Rüdiger Hülsmann	12.10.2009	Added possibility of idle speed control
'- Rüdiger Hülsmann	11.05.2010	Added "E-Gas" function (throttle override by stop brake)
'- Rüdiger Hülsmann	13.05.2010	Added engine temperature and cooling system
'- Rüdiger Hülsmann	08.07.2010	Bugfix E-Gas
'- Rüdiger Hülsmann	06.11.2010	Improved engine start and stop procedure 
'- Marcel Kuhnt		09.11.2010	refueling included
'- Rüdiger Hülsmann	21.11.2010	thermostat short circuit
'- Rüdiger Hülsmann	22.11.2010	engine coolable by fan heaters
'- Rüdiger Hülsmann	24.12.2010	optional ASR (traction control)
'- Rüdiger Hülsmann	29.12.2010	ASR debugged
'- Rüdiger Hülsmann	01.01.2011	ASR debugged again
'- Rüdiger Hülsmann	05.01.2011	20h-switch E-Gas
'- Marcel Kuhnt		07.01.2011	writing tank_percent variable
'- Rüdiger Hülsmann	10.01.2011	Internal throttle set to 0 during shutdown
'- Rüdiger Hülsmann	23.01.2011	ASR relais sound
'- Kyle Ortiz	        05.07.2011	Added turbochager
'- Kyle Ortiz	        30.07.2011	Added Speed Governer with RPM governer while the bus is in drive
'- Kyle Ortiz	        16.08.2011	Changed engine braking algorithm. 
'- Kyle Ortiz	        16.12.2011	Added nemeza's fuel code.
'- Kyle Ortiz	        20.8.2012-5.10.2012	Changed turbochager Characteristic



'------------------------------------------------------------------------------------------


'----------------------
'	Trigger
'----------------------

{trigger:kw_m_engine_startbutton}
	(L.L.engine_on) ! (L.L.antrieb_getr_gangwahl) 1 = (L.L.elec_busbar_main) && &&
	{if}
		1 (S.L.engine_on) (S.L.engine_injection_on)
		(T.L.ev_enginestart)
		300 (S.L.engine_n)
	{endif}	
	1 (S.L.cp_taster_anlasser)
{end}

{trigger:kw_m_engine_startbutton_off}
	0 (S.L.cp_taster_anlasser)
{end}

{trigger:kw_m_enginestart}
	(L.L.engine_starter_antirepeat) !
	{if}
		(L.L.engine_on) !
		{if}	
			(L.L.antrieb_getr_gangwahl) 1 = (L.L.elec_busbar_main) && 
			{if}
				1 (S.L.engine_on) (S.L.engine_injection_on)
				(T.L.ev_enginestart)
				300 (S.L.engine_n)
			{endif}	
			1 (S.L.cp_taster_anlasser) (S.L.engine_starter_antirepeat)
		{else}
			(L.L.elec_busbar_main)
			{if}
				0 (S.L.engine_injection_on)
				1 (S.L.engine_starter_antirepeat)
			{endif}
			1 (S.L.cp_taster_motorabstellung)
		{endif}
	{endif}

{end}

{trigger:kw_m_enginestart_off}
	0 (S.L.cp_taster_motorabstellung) (S.L.cp_taster_anlasser) (S.L.engine_starter_antirepeat)
	1 (S.L.engine_injection_on)
{end}


{trigger:kw_m_engineshutdown}
	(L.L.elec_busbar_main)
	{if}
		0 (S.L.engine_injection_on)
	{endif}
	1 (S.L.cp_taster_motorabstellung)
{end}

{trigger:kw_m_engineshutdown_off}
	0 (S.L.cp_taster_motorabstellung)
	1 (S.L.engine_injection_on)
{end}

{trigger:veh_tank}
	(L.L.engine_tank_content) (L.S.Timegap) 3 * + (C.L.engine_tank_capacity) min (S.L.engine_tank_content)
{end}

{macro:engine_init}

	50 50 (C.L.engine_tank_capacity) - random + (S.L.engine_tank_content)
	(L.S.Weather_Temperature) (S.L.engine_temperature) (S.L.engine_temperature_envir)
{end}


{macro:engine_frame}

	(M.L.speed_governor)

	(L.L.engine_last_n) 300 >=
	(L.L.engine_n) 300 < &&
	{if}
		(M.L.engine_stall)
		0 (S.L.engine_on)
	{endif}
	
	
	(L.L.engine_n) (S.L.engine_last_n)

	
	(L.L.engine_n) 100 < (L.L.engine_injection_on) ! &&
	{if}
		0 (S.L.engine_n) 
	{endif}

	(L.L.bremse_kompressor)	(L.L.engine_on) &&
	{if}	
		10 (S.L.engine_M_additional_load)
	{else}
		0 (S.L.engine_M_additional_load)
	{endif}

	(M.L.engine_temperature)

	(M.L.engine_consumption)

	(M.L.turbochanger)

	

(L.L.engine_M) (L.L.engine_n) (F.L.engine_M_maxThrottle) / (S.L.engine_output)
	
	
	
	(L.L.antrieb_Torque_Governor_ADJ) (L.L.engine_n) (F.L.engine_M_maxThrottle) (L.L.throttle) * / 1 max s1

	(L.L.throttle) (L.L.antrieb_getr_debug2) l1 * * (S.L.engine_internal_throttle)

'	Override durch Haltestellenbremse ODER Motorabstellung

	(L.L.bremse_halte_sw) (L.L.door_20h_sw) || (C.L.engine_e-gas) &&
	(L.L.engine_injection_on) ! || 
	{if}
		0 (S.L.engine_internal_throttle)
	{endif}

	(C.L.engine_speedcontrol)
	{if}
		(M.L.engine_speedcontrol)
	{endif}

'MCQ: calculating tank content percent and write into pre defined variable for publishing on red line:


'	Motormanagement durch ASR-Eingriff, sofern vorhanden

	(L.L.elec_busbar_main) &&
	{if}
		(L.L.Wheel_RotationSpeed_1_L) (L.L.Wheel_RotationSpeed_1_R) + 2 / abs (L.L.Wheel_RotationSpeed_0_L) (L.L.Wheel_RotationSpeed_0_R) + 1 / 10 + abs >
		(L.L.Wheel_RotationSpeed_1_L) 1 > &&
		(L.L.Wheel_RotationSpeed_1_R) 1 > &&
		(L.L.engine_internal_throttle) 0 > &&
		{if}
			(L.L.engine_ASR_eingriff) !
			{if}
				(T.L.ev_bremse_ABS_0R_on)
			{endif}	
			1 (S.L.engine_ASR_eingriff)
		{endif}
		(L.L.Wheel_RotationSpeed_1_L) (L.L.Wheel_RotationSpeed_1_R) + 2 / abs (L.L.Wheel_RotationSpeed_0_L) (L.L.Wheel_RotationSpeed_0_R) + 2 / 8 + abs <
		{if}
			(L.L.engine_ASR_eingriff)
			{if}
				(T.L.ev_bremse_ABS_0R_off)
			{endif}	
			0 (S.L.engine_ASR_eingriff)
		{endif}

		(L.L.engine_ASR_eingriff)
		{if}
			0 (S.L.engine_internal_throttle)
		{endif}

	{else}
'		Wenn ASR aus, dann Dauerleuchten
		(L.L.elec_busbar_main) 
		{if}
			(L.L.engine_ASR_eingriff) !
			{if}
				(T.L.ev_bremse_ABS_0R_on)
			{endif}	
			1 (S.L.engine_ASR_eingriff)
		{else}
			(L.L.engine_ASR_eingriff)
			{if}
				(T.L.ev_bremse_ABS_0R_off)
			{endif}	
			0 (S.L.engine_ASR_eingriff)
		{endif}
	{endif}


	
{end}


{macro:engine_moment}

	
	(L.L.Velocity) (C.L.speedgov) - (F.L.governor) (S.L.engine_spdgov)
 

	(L.L.antrieb_getr_aktugang) 0 > (L.L.antrieb_getr_fest) &&
	{if}
		(L.L.engine_n) (C.L.rpmgov) - (F.L.rpmgov_map) (S.L.RPM_Governor)
	{else}
		(L.L.engine_n) 2650 - (F.L.rpmgov_map) (S.L.RPM_Governor)
	{endif}

	(L.L.engine_internal_throttle) (L.L.engine_spdgov) (L.L.RPM_Governor) * min (S.L.engine_internal_throttle)

	 (L.L.Torque_Governor_set) 0 =

	 {if}
	(L.L.engine_n) (F.L.engine_M_maxThrottle) s5
	 {else}
	   (L.L.Torque_Governor_set) s5
	 {endif}

			    
	  (L.L.engine_n) (F.L.engine_M_maxThrottle) (L.L.Torque_Governor_ADJ) >
	     {if}

	   (L.L.engine_n) (F.L.engine_M_maxThrottle) (S.L.Torque_Governor_ADJ)

	    {endif}	
			      
'Calculate transmission settings 


	(L.L.Torque_Governor_set) (L.L.antrieb_getr_aktugang) &&
	{if}
		  (C.L.engine_ECM_Throttle)
		   {if}
		 (L.L.engine_M) (L.L.Torque_Governor_set) (L.L.throttle) * / (F.L.Torque_Requested_Map) s6  (S.L.antrieb_getr_debug2)
		    	{else}
			 1 (S.L.antrieb_getr_debug2) s6
		    {endif}

		 (L.L.Torque_Governor_set) (S.L.antrieb_Torque_Governor_ADJ) (L.L.throttle) l6 * *  (L.L.engine_n) (F.L.engine_M_maxThrottle)  / 0 max 0.999 min  (S.L.Torque_Governor)
	{else}
		  (C.L.engine_ECM_Throttle)
		   {if}
		(L.L.engine_M) (S.L.antrieb_Torque_Governor_ADJ) (L.L.Torque_Governor_ADJ) (L.L.throttle) * / (F.L.Torque_Requested_Map) s6  (S.L.antrieb_getr_debug2) s6
			    	{else}
			 1 (S.L.antrieb_getr_debug2) s6
		    {endif}

		 (L.L.Torque_Governor_ADJ) (L.L.throttle) l6 * * (L.L.engine_n) (F.L.engine_M_maxThrottle)  / 0 max 0.999 min  (S.L.Torque_Governor)

	
	{endif}

	

'	Reaktionszeit der Einspritzpumpe
	(L.L.engine_internal_throttle) (L.L.engine_throttle_injection) >
	{if}
		(L.L.engine_throttle_injection) (L.S.Timegap) 4 * + (L.L.engine_internal_throttle)  min (S.L.engine_throttle_injection)
	{else}
		(L.L.engine_throttle_injection) (L.S.Timegap) 4 * - (L.L.engine_internal_throttle) max (S.L.engine_throttle_injection)
	{endif}
 	
	(L.L.engine_throttle_injection) (L.L.Torque_Governor) min (S.L.engine_throttle_injection)	
		
	
' Throttle Controller

	  
	(L.L.engine_injection_on) (L.L.engine_on) &&
	{if}

	(C.L.turbochaged) (L.L.engine_throttle_injection) 0.1 > &&
	{if}

		
		 (C.L.engine_CID) (L.L.engine_n) * 80 * 5660 / 14.7 (L.L.turbo_psi) + 14.7 / *  (S.L.engine_airflow)

		 (L.L.engine_airflow) (F.L.turbo_exhaust_flow) (L.L.engine_throttle_injection) * (C.L.turbo_max_psi) (L.L.engine_throttle_injection) * min (S.L.turbo_limit_thorttle) 

'			Regulates the amount of turbocharger boost based on throttle position 

		(C.L.turbo_max_psi) (C.L.turbo_compressor_wheel_size) sqr 14.7 (L.L.turbo_psi) + 80 * / / s1 

		 (L.L.turbo_psi) 0.6 * s5
		   (L.L.engine_n) 1260 <
		   {if}

		   (L.L.turbo_psi) (F.L.turbo_spool_oj) s6 
		   {else}
		      1 s6

		  {endif}

     		  (C.L.engine_ECM_Throttle)
		   {if}
		   	 1 s2
		    {else}
		     
		       (L.L.engine_throttle_injection) s2
		   {endif}


		(L.L.turbo_limit_thorttle) (L.L.turbo_psi) >
		{if}	
			
			(L.L.turbo_psi) (L.S.Timegap) l1 l6 l2 * * * +  (C.L.turbo_max_psi) 0.99 (L.L.engine_throttle_injection) * * min (S.L.turbo_psi)

		{endif}

		(L.L.turbo_limit_thorttle) (L.L.turbo_psi) <
		{if}	
			(L.L.turbo_psi) (L.S.Timegap) l1 * - (C.L.turbo_min_psi) max (S.L.turbo_psi)

		{endif}

'Units are in English (PSI) not Metric 
		

		     (L.L.turbo_psi) (C.L.turbo_max_psi) / 0 max 1 min (S.L.turbo_debug_1)

		

	

		    (L.L.engine_n) (F.L.engine_M_maxThrottle) 14.7 (C.L.turbo_max_psi) 14.7 + / * (S.L.enginena_M)


		    1 14.7 (C.L.turbo_max_psi) 14.7 + / - (S.L.turbo_M)
		   (L.L.turbo_debug_1) (L.L.engine_n) (F.L.engine_M_maxThrottle) (L.L.turbo_M) * * (S.L.engineNA1_M)
		   (L.L.enginena_M) (S.L.engine_resultant_M)  
	{else}
		(C.L.turbo_max_psi) (C.L.turbo_compressor_wheel_size) sqr 14.7 (L.L.turbo_psi) + 80 * / / s1 
		(L.L.turbo_psi) (L.S.Timegap) l1 * - (C.L.turbo_min_psi) max (S.L.turbo_psi)

		(L.L.engine_n) (F.L.engine_M_maxThrottle) (S.L.engine_resultant_M)
		0 (S.L.engineNA1_M) 
		1 (S.L.turbo_M)
		{endif}
		

		(L.L.engine_throttle_injection) s1 (L.L.engine_resultant_M) * 1 l1 - (L.L.engine_n) (F.L.engine_M_minThrottle) (L.L.engine_throttle_injection) (F.L.engine_brake_fadin) * * + (L.L.engineNA1_M)  + (S.L.engine_M)
	
	{else}
		(L.L.engine_n) 1 >
		{if}
			(C.L.engine_coldM) (S.L.engine_M)
		{else}
			0 (S.L.engine_M)
			0 (S.L.turbo_psi)
		{endif}
	{endif}

{end}


{macro:turbochanger}	


	

	
		
{end}


{macro:engine_acceleration}


'	Berechnung der Drehzahlbeschleunigung:
' 	Calculation of speed acceleration:

	(L.L.engine_M) (L.L.antrieb_getr_M_an) (L.L.engine_M_additional_load) + - (C.L.engine_J) /

'	... Berechnung der Motordrehzahl anhand der Drehzahlbeschleunigung:

	(L.S.Timegap) * 30 * pi / (L.L.engine_n) + (S.L.engine_n)
{end}





{macro:engine_consumption}
'					      	=2*PI/60
	(L.L.engine_M) 0 max (L.L.engine_n) * 0.10472 * s0
	(L.L.engine_on)
	{if}
		l0 (C.L.engine_power_idle) + (S.L.engine_power)
	{else}
		l0 (S.L.engine_power)
	{endif}
	
	(L.L.engine_energytransfer) (L.L.engine_power) (L.S.Timegap) * 1000 / 3600 / + (S.L.engine_energytransfer)
	(L.L.engine_energy_used) (L.L.engine_power) (L.S.Timegap) * 1000 / 3600 / (L.L.engine_n) (F.L.engine_efficiency_rpm) (L.L.engine_throttle_injection) (F.L.engine_efficiency_throttle) / / s0 + (S.L.engine_energy_used)

	(C.L.engine_consumption_curve_available)
	{if}
		(L.L.engine_n) (F.L.engine_consumption_per_rpm) 1000 / s2
		1 l2 / 0.845 * s2
		(L.L.engine_fuel_used) l0 l2 / s1 + (S.L.engine_fuel_used)
	{else}
		(L.L.engine_fuel_used) l0 (C.L.engine_fuel_value) / s1 + (S.L.engine_fuel_used)
	{endif}

		(L.L.engine_tank_content) (C.L.engine_tank_capacity) / (S.L.tank_percent)
	
	l1 (L.S.Timegap) / 3600 * (S.L.engine_consumption_h)

	(L.L.engine_tank_content) l1 - 0 max (S.L.engine_tank_content)
	0 <= 
	(L.L.engine_failure_general) ||
	{if}
		0 (S.L.engine_on)
	{endif}



	
{end}

{macro:engine_stall}
	
	(T.L.ev_engineshutdown)
	
	0 (S.L.engine_on) 
{end}

{macro:engine_speedcontrol}

	(L.L.engine_n) (C.L.engine_governed_idle_RPM) <
	{if}
		(L.L.engine_additional_throttle) (L.S.Timegap) 0.2 * + (S.L.engine_additional_throttle)
	{else}
		(L.L.engine_additional_throttle) (L.S.Timegap) 0.2 * - 0 max (S.L.engine_additional_throttle)
	{endif}

	(L.L.engine_internal_throttle) (L.L.engine_additional_throttle) + 1 min 0 max (S.L.engine_internal_throttle)

{end}
{macro:speed_governor}



 
{end}


{macro:engine_temperature}


	(L.L.engine_power) (C.L.engine_Qrate_engine_factor) * (S.L.engine_Qrate_engine)


	(L.L.elec_busbar_main) (L.L.engine_on) &&
	{if}
		(L.L.engine_temperature) (C.L.luefterthermostat_opn) >
		(L.L.cp_motorkuehlung_sw) ||
		{if}
			1 (S.L.engine_luefter)
		{else}
			(L.L.engine_temperature) (C.L.luefterthermostat_cls) <
			(L.L.cp_motorkuehlung_sw) ! &&
			{if}
			0 (S.L.engine_luefter)
			{endif}
		{endif}
	{else}
		0 (S.L.engine_luefter)
	{endif}

	(L.L.engine_temperature) (C.L.kuehlerthermostat_opn) >
	{if}
		1 (S.L.engine_thermostat_open)
	{else}
		(L.L.engine_temperature) (C.L.kuehlerthermostat_cls) <
		{if}
			0 (S.L.engine_thermostat_open)
		{endif}
	{endif}

	
'	--------------------------------------------------
'	Berechnung der Raten:

	(L.L.engine_temperature) (L.L.engine_temperature_envir) - (C.L.engine_Qrate_cooling_factor) * (S.L.engine_Qrate_cooling)
	(L.L.engine_temperature_envir) (L.S.Weather_Temperature) - (C.L.engine_Qrate_Veloc_factor_basic) (C.L.engine_Qrate_veloc_factor) (L.L.velocity) abs * + * (S.L.engine_Qrate_veloc)

	(L.L.engine_temperature) (L.S.Weather_Temperature) - (C.L.engine_Qrate_fan_factor) * (L.L.engine_n) * (S.L.engine_Qrate_fan)


	(L.L.engine_thermostat_open)
	{if}
		(L.L.engine_luefter) !
		{if}	
'			Reduktion der Kühlwirkung durch nur leer mitdrehenden Lüfter
			(L.L.engine_Qrate_fan) 0.4 * (S.L.engine_Qrate_fan)	
		{endif}
	{else}			
'		Nullwirkung des Lüfters durch Kühlwasserkurzschluss	
		0 (S.L.engine_Qrate_fan)
	{endif}


'	--------------------------------------------------
'	Berechnung der Temperaturveränderungen:

	(L.L.engine_Qrate_engine) (L.L.engine_Qrate_cooling) - (L.L.engine_Qrate_fan) - (L.L.cabinair_Qrate_engine_fanheatcooling) - (C.L.engine_cvm_engine) / (L.S.Timegap) * (L.L.engine_temperature) + (S.L.engine_temperature) 
	(L.L.engine_Qrate_cooling) (L.L.engine_Qrate_veloc) - (C.L.engine_cvm_envir) / (L.S.Timegap) * (L.L.engine_temperature_envir) + (S.L.engine_temperature_envir) 


'--------------------------------------------------




'	Kochendes Kühlwasser
	(L.L.engine_temperature) (F.L.kuehlwassersmoke) (S.L.engine_kuehlwasser_freq)


	

	
{end}


